\*\*This is the driver for the Knoxi Brand **G-sensor.**

For example, it is G-sensor for the QW1012 10.1inch Tablet PC.

Step by step:

1) Install “kxaccel-1.0.13.20-win8-x86” firstly, after installed successfully, restart the Tablet PC.

2) After the Tablet PC was restarted, double click “kionix\_sensor\_orientation” to enroll it into the regedit. Restart the Tablet PC.